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Warning
 
 
 
 

SECTION 1: Identification of the substance/mixture and of the company/undertaking 
1.1. Product identifier 
	Trade name 
	: Carbon dioxide 

	SDS no 
	: EIGA018A-ALBNL 

	Other means of identification 
	: Carbon dioxide 

	 
		CAS-No. 	: 124-38-9 

	 
		EC-No. 	: 204-696-9 

	 
 
		EC Index-No. 	: --- 

	REACH registration No 
 
	: Listed in Annex IV / V REACH, exempted from registration. 

	Chemical formula 
	: CO2 


1.2. Relevant identified uses of the substance or mixture and uses advised against 
Relevant identified uses 	: Extinguishing agent. 
Industrial and professional uses. Perform risk assessment prior to use. 
Test gas/Calibration gas. 
Purge gas, diluting gas, inerting gas. 
Shield gas for welding processes. 
Use for manufacture of electronic/photovoltaic components. 
Consumer use. 
Treatment of water intended for human consumption. 
It is the responsibility of the end user to ensure that the product as supplied is suitable for its intended use. 
Uses advised against 	: None. 
1.3. Details of the supplier of the safety data sheet 
BELGIUM: 
Janox BV
Roggestraat 12
8972 Krombeke
Belgium-Belgique-België 
Tel: +32 (0)57 30 98 40
info@janox.be

1.4. Emergency telephone number 
	Country/Area 
	Organisation/Company 
	Address 
	Emergency number 
	Comment 

	Belgium 
	Centre Anti-Poisons/Antigifcentrum c/o Hôpital Militaire Reine Astrid 
	Rue Bruyn 1 
1120 Bruxelles/Brussel  
	+32 70 245 245 
	Please dial: 070 245 245 for any urgent questions about intoxication 
(free of charge 24/7), if not accessible, dial: 02 264 96 30 
(standard fee) 

	Luxembourg 
	Centre Anti-Poisons/Antigifcentrum c/o Hôpital Militaire Reine Astrid 
	Rue Bruyn 1 
1120 Bruxelles/Brussel  
	+352 8002 5500 
	Free telephone number with a 24/7 access. Experts answer all urgency questions on dangerous products in French, Dutch and English 

	Netherlands 
	Nationaal Vergiftigingen Informatie 
Centrum 
	Huispostnummer 
Q03.2.315 
Postbus 85500 
3508 GA Utrecht  
	+31 88 755 80 00 
	Only for the purpose of informing medical personnel in cases of acute intoxications (24 hours a day, 7 days a week) 


SECTION 2: Hazards identification 
2.1. Classification of the substance or mixture 
Classification according to Regulation (EC) No. 1272/2008 [CLP] 
Physical hazards 	Gases under pressure : Liquefied gas 	H280 	 
2.2. Label elements 
Labelling according to Regulation (EC) No. 1272/2008 [CLP] 
[image: ]Hazard pictograms (CLP) 	:  	 	 	 	 
 
	
	GHS04 

	Signal word (CLP) 
	: Warning 

	Hazard statements (CLP) 
	: H280 - Contains gas under pressure; may explode if heated. 

	Precautionary statements (CLP) 
	  

	- Storage 
	: P403 - Store in a well-ventilated place. 

	Supplemental information 
	: Asphyxiant in high concentrations. 
Contains fluorinated greenhouse gases. 


2.3. Other hazards 
 	 Contact with liquid may cause cold burns/frostbite. 
In high concentrations CO2 causes rapid circulatory insufficiency even at normal levels of oxygen concentration. Symptoms are headache, nausea and vomiting, which may lead to unconsciousness and death. 
Not classified as PBT or vPvB. 
The substance/mixture has no endocrine disrupting properties. 
Not classified as PMT or vPvM. 
SECTION 3: Composition/information on ingredients 
3.1. Substances 	  
 
	Name 
	Product identifier 
	% 
	Classification according to Regulation 
(EC) No. 1272/2008 [CLP] 
ATE, EUH-statements, M-Factors 

	Carbon dioxide 
	CAS-No.: 124-38-9 
EC-No.: 204-696-9 
EC Index-No.: --- 
REACH registration No: *1 
	100 
	Press. Gas (Liq.), H280 


 
 
Full text of H- and EUH-statements: see section 16 
Contains no other components or impurities which will influence the classification of the product. 
*1: Listed in Annex IV / V REACH, exempted from registration. 
*3: Registration not required: Substance manufactured or imported < 1t/y. 
3.2. Mixtures 	 Not applicable 
SECTION 4: First aid measures 
4.1. Description of first aid measures 
· Inhalation 	: Remove victim to uncontaminated area wearing self contained breathing apparatus. Keep 
victim warm and rested. Call a doctor. Perform cardiopulmonary resuscitation if breathing stopped. 
· Skin contact 	: In case of frostbite spray with water for at least 15 minutes. Apply a sterile dressing. Obtain medical assistance. 
· Eye contact 	: Immediately flush eyes thoroughly with water for at least 15 minutes. - Ingestion 	: Ingestion is not considered a potential route of exposure. 
4.2. Most important symptoms and effects, both acute and delayed 
 	 In high concentrations may cause asphyxiation. Symptoms may include loss of 
mobility/consciousness. Victim may not be aware of asphyxiation. 
Low concentrations of CO2 cause increased respiration and headache. See section 11. 
4.3. Indication of any immediate medical attention and special treatment needed 
 	 None. 
SECTION 5: Firefighting measures 
5.1. Extinguishing media 
· Suitable extinguishing media 	: Water spray or fog. 
Product does not burn, use fire control measures appropriate for the surrounding fire. 
· Unsuitable extinguishing media 	: Do not use water jet to extinguish. 
5.2. Special hazards arising from the substance or mixture 
	Specific hazards 
	: Exposure to fire may cause containers to rupture/explode. 

	Hazardous combustion products 
5.3. Advice for firefighters 
	: None. 

	Specific methods 
	: Use fire control measures appropriate for the surrounding fire. Exposure to fire and heat radiation may cause gas receptacles to rupture. Cool endangered receptacles with water spray jet from a protected position. Prevent water used in emergency cases from entering sewers and drainage systems. 
If possible, stop flow of product. 
Use water spray or fog to knock down fire fumes if possible. 
Move containers away from the fire area if this can be done without risk. 

	Special protective equipment for fire fighters 
	: In confined space use self-contained breathing apparatus. 
Standard protective clothing and equipment (Self Contained Breathing Apparatus) for fire fighters. 
Standard EN 137 - Self-contained open-circuit compressed air breathing apparatus with full face mask. 
Standard EN 469 - Protective clothing for firefighters. Standard - EN 659: Protective gloves for firefighters. EN 15090 Footwear for firefighters. EN 443 Helmets for fire fighting in buildings and other structures. 


SECTION 6: Accidental release measures 
6.1. Personal precautions, protective equipment and emergency procedures 
	For non-emergency personnel 
	: Act in accordance with local emergency plan. 
Try to stop release. 
Evacuate area. 
Ensure adequate air ventilation. 
Prevent from entering sewers, basements and workpits, or any place where its accumulation can be dangerous. 
Stay upwind. 
See section 8 of the SDS for more information on personal protective equipment. 

	For emergency responders 6.2. Environmental precautions 
	: Wear self-contained breathing apparatus when entering area unless atmosphere is proved to be safe. 
Oxygen detectors should be used when asphyxiating gases may be released. 
See section 5.3 of the SDS for more information. 

	 
	 Try to stop release. 


6.3. Methods and material for containment and cleaning up 
 	 Ventilate area. 
6.4. Reference to other sections 
 	 See also sections 8 and 13. 
SECTION 7: Handling and storage 
7.1. Precautions for safe handling 
	Safe use of the product 
	: Containers, which contain or have contained flammable or explosive substances, must not be inerted with liquid carbon dioxide. Potential production of solid CO2 particles must be ruled out. In order to rule out potential electrostatic discharge production, the system must be adequately grounded. 
Do not breathe gas. 
Avoid release of product into atmosphere. 
The product must be handled in accordance with good industrial hygiene and safety procedures. 
Only experienced and properly instructed persons should handle  gases under pressure. 
Consider pressure relief device(s) in gas installations. 
Ensure the complete gas system was (or is regularily) checked for leaks before use. 
Do not smoke while handling product. 
Use only properly specified equipment which is suitable for this product, its supply pressure and temperature. Contact your gas supplier if in doubt. 
Avoid suck back of water, acid and alkalis. 
Be aware of the risk of formation of static electricity with the use of CO2 extinguishers. Do not use them in places where a flammable atmosphere may be present. 

	Safe handling of the gas receptacle 
	: Do not allow backfeed into the container. 
Protect containers from physical damage; do not drag, roll, slide or drop. 
When moving cylinders, even for short distances, use a cart (trolley, hand truck, etc.) designed to transport cylinders. 
Leave valve protection caps, when provided, in place until the container has been secured against either a wall or bench or placed in a container stand and is ready for use. 
If user experiences any difficulty operating valve discontinue use and contact supplier. 
Never attempt to repair or modify container valves or safety relief devices. 
Damaged valves should be reported immediately to the supplier. 
Keep container valve outlets clean and free from contaminants particularly oil and water. Replace valve outlet caps or plugs and container caps where supplied as soon as container is disconnected from equipment. 
Close container valve after each use and when empty, even if still connected to equipment. 
Never attempt to transfer gases from one cylinder/container to another. 
Never use direct flame or electrical heating devices to raise the pressure of a container. Do not remove or deface labels provided by the supplier for the identification of the content of the container. 
Suck back of water into the container must be prevented. 
Open valve slowly to avoid pressure shock. 


7.2. Conditions for safe storage, including any incompatibilities 
 	 Observe all regulations and local requirements regarding storage of containers. 
Containers should not be stored in conditions likely to encourage corrosion. 
Container valve guards or caps, when provided, should be in place. 
Containers should be stored in the vertical position and properly secured to prevent them from falling over. 
Stored containers should be periodically checked for general condition and leakage. 
Keep container below 50°C in a well ventilated place. 
Store containers in location free from fire risk and away from sources of heat and ignition. Keep away from combustible materials. 
7.3. Specific end use(s) 
 	 None. 
SECTION 8: Exposure controls/personal protection 
8.1. Control parameters 
	Carbon dioxide (124-38-9) 
	

	EU - Indicative Occupational Exposure Limit (IOEL) 
	

	Local name 
	Carbon dioxide 

	IOEL TWA 
	9000 mg/m³ 

	
	5000 ppm 

	Regulatory reference 
	COMMISSION DIRECTIVE 2006/15/EC 

	Belgium - Occupational Exposure Limits 
	

	Local name 
	Carbone (dioxyde de) # Koolstofdioxide 

	OEL TWA 
	9131 mg/m³ 

	
	5000 ppm 

	OEL STEL 
	54784 mg/m³ 

	
	30000 ppm 

	Remark 
	A: la mention “A” signifie que l’agent libère un gaz ou une vapeur qui n’ont en eux-mêmes aucun effet physiologique mais peuvent diminuer le taux d’oxygène dans l’air. Lorsque le taux d’oxygène descend en dessous de 1718 % (vol/vol) le manque d’oxygène provoque des suffocations qu’aucun symptôme préalable n’annonce. # A: de vermelding “A” betekent dat dit agens gas of damp vrijgeeft dat of die op zich geen fysiologische werking heeft, maar het zuurstofgehalte in de lucht verlaagt. Wanneer het zuurstofgehalte daalt onder de 17-18 % (vol/vol), veroorzaakt het zuurstoftekort verstikking, die zich manifesteert zonder dat er een waarschuwing aan voorafgaat. 

	Regulatory reference 
	Koninklijk besluit/Arrêté royal 16/11/2023 

	Luxembourg - Occupational Exposure Limits 
	

	Local name 
	Dioxyde de carbone 

	OEL TWA 
	9000 mg/m³ 

	
	5000 ppm 

	Regulatory reference 
	Mémorial A Nº 226 de 2021 concernant la protection de la sécurité et de la santé des salariés contre les risques liés à des agents chimiques sur le lieu de travail 

	Netherlands - Occupational Exposure Limits 
	

	Local name 
	Kooldioxide 

	TGG-8u (OEL TWA) 
	9000 mg/m³ 

	
	5000 ppm 

	Regulatory reference 
	Arbeidsomstandighedenregeling 2024 


 
	DNEL (Derived-No Effect Level) 
 
	: None available. 

	PNEC (Predicted No-Effect Concentration) 
	: None available. 


8.2. Exposure controls 
8.2.1. Appropriate engineering controls 
 	 Provide adequate general and local exhaust ventilation. 
Systems under pressure  should be regularily checked for leakages. 
Ensure exposure is below occupational exposure limits (where available). 
Oxygen detectors should be used when asphyxiating gases may be released. 
Consider the use of a work permit system e.g. for maintenance activities. CO2 detectors should be used when CO2 may be released. 
8.2.2. Individual protection measures, e.g. personal protective equipment 
 	 A risk assessment should be conducted and documented in each work area to assess the 
risks related to the use of the product and to select the PPE that matches the relevant risk. 
The following recommendations should be considered: 
PPE compliant to the recommended EN/ISO standards should be selected. 
· Eye/face protection 	: Wear goggles when transfilling or breaking transfer connections. 
Standard EN 166 - Personal eye-protection - specifications. 
· Skin protection 	 	 
· Hand protection 	: Wear working gloves when handling gas containers. 
Standard EN 388 - Protective gloves against mechanical risks, performance level 1 or higher. Recommended types include wrist gloves from leather or synthetic material with equivalent performance, fabric gloves, fabric gloves with leather palms. 
Wear cold insulating gloves when transfilling or breaking transfer connections. 
Standard EN 511 - Cold insulating gloves, performance level 1 or higher. Recommended types include insulated gauntlets or gloves specifically selected to prevent liquid penetration and ingress of cryogenic liquids and to provide mechanical resistance. 
· Other 	: Wear safety shoes while handling containers. 
Standard EN ISO 20345 - Personal protective equipment - Safety footwear. 
· Respiratory protection 	: Standard EN 137 - Self-contained open-circuit compressed air breathing apparatus with full face mask. 
Consult respiratory device supplier´s product information for the selection of the appropriate device. 
Self contained breathing apparatus (SCBA) or positive pressure airline with mask are to be used in oxygen-deficient atmospheres. 
Self contained breathing apparatus is recommended, where unknown exposure may be expected, e.g. during maintenance activities on installation systems. 
· Thermal hazards 	: None in addition to the above sections. 
8.2.3. Environmental exposure controls 
 	 None necessary. 
SECTION 9: Physical and chemical properties 
9.1. Information on basic physical and chemical properties 
	Appearance 
	 	 

	     - Physical state at 20°C / 101.3kPa 
	: Gas. 

	     - Colour 
	: Colourless. 

	Odour 
	: Odourless. 

	Melting point / Freezing point 
	: -78,5 °C Melting point at normal conditions does not exist. At atmospheric pressure solid carbon dioxide sublimes into gaseous carbon dioxide at -78.5°C 

	Boiling point 
	: -56,6 °C 

	Flammability 
	: Non flammable. 

	Lower explosion limit 
	: Not applicable. 

	Upper explosion limit 
	: Not applicable. 

	Flash point 
	: Not applicable for gases and gas mixtures. 

	Auto-ignition temperature 
	: Non flammable. 

	Decomposition temperature 
	: Not applicable. 

	pH 
	: Not applicable for gases and gas mixtures. 

	Viscosity, kinematic 
	: Not applicable for gases and gas mixtures. 

	Water solubility [20°C] 
	: 2000 mg/l 


Partition coefficient n-octanol/water (Log Kow) 	: 0,83 
Vapour pressure [20°C] 	: 57,3 bar(a) 
Vapour pressure [50°C] 	: No reliable data available. 
Density and/or relative density 	: Not applicable for gases and gas mixtures. 
Relative vapour density (air=1) 	: 1,52 
Particle characteristics 	: Not applicable for gases and gas mixtures. 
Nanoforms are not relevant for gases and gas mixtures. 
 
9.2. Other information 
9.2.1. Information with regard to physical hazard classes 
	Oxidising properties 
	: No oxidising properties. 

	Critical temperature [°C] 
9.2.2. Other safety characteristics 
	: 31 °C 

	Molar mass 
	: 44 g/mol 

	Other data 
	: Gas/vapour heavier than air. May accumulate in confined spaces, particularly at or below ground level.  


SECTION 10: Stability and reactivity 
10.1. Reactivity 
 	 No reactivity hazard other than the effects described in sub-sections below. 
10.2. Chemical stability 
 	 Stable under normal conditions. 
10.3. Possibility of hazardous reactions 
 	 None. 
10.4. Conditions to avoid 
 	 Avoid moisture in installation systems. 
10.5. Incompatible materials 
 	 For additional information on compatibility refer to ISO 11114. 
10.6. Hazardous decomposition products 
 	 None. 
 SECTION 11: Toxicological information 
11.1. Information on hazard classes as defined in Regulation (EC) No 1272/2008 
	Acute toxicity 
 
	: Toxicological effects not expected  by inhalation from this product if occupational exposure limit values are not exceeded. 

	Skin corrosion/irritation 
 
	: No known effects from this product. 

	Serious eye damage/irritation 
 
	: No known effects from this product. 

	Respiratory or skin sensitisation 
 
	: No known effects from this product. 

	Germ cell mutagenicity 
 
	: No known effects from this product. 

	Carcinogenicity 
 
	: No known effects from this product. 

	Toxic for reproduction : Fertility 
	: No known effects from this product. 

	Toxic for reproduction : unborn child 
 
	: No known effects from this product. 

	STOT-single exposure 
 
	: No known effects from this product. 

	STOT-repeated exposure 
	: No known effects from this product. 
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	Aspiration hazard 
11.2. Information on other hazards 
	Not applicable for gases and gas mixtures. 

	Other information 
	: Unlike simple asphyxiants, carbon dioxide has the ability to cause death even when normal oxygen levels (20-21%) are maintained. 5% CO2 has been found to act synergistically to increase the toxicity of certain other gases (CO, NO2). CO2 has been shown to enhance the production of carboxy- or met-hemoglobin by these gases possibly due to carbon dioxide’s stimulatory effects on the respiratory and circulatory systems. 
For more information, see 'EIGA Safety Info 24: Carbon Dioxide, Physiological Hazards' at www.eiga.eu. 
The substance/mixture has no endocrine disrupting properties. 

	SECTION 12: Ecological information 
	
	

	12.1. Toxicity 
 
Assessment 
 
	: 
	No ecological damage caused by this product. 

	 
EC50 48h - Daphnia magna [mg/l] 
	: 
	No data available. 

	EC50 72h - Algae [mg/l] 
	: 
	No data available. 

	LC50 96 h - Fish [mg/l] 
	: 
	No data available. 

	12.2. Persistence and degradability 
Assessment 
	: 
	No ecological damage caused by this product. 

	12.3. Bioaccumulative potential 
Assessment 
	: 
	No ecological damage caused by this product. 
Not expected to bioaccumulate due to the low log Kow (log Kow < 4). See section 9. 

	12.4. Mobility in soil 
Assessment 
	: 
	No ecological damage caused by this product. 

	12.5. Results of PBT and vPvB assessment 
Assessment 
	: 
	Not classified as PBT or vPvB. 

	12.6. Endocrine disrupting properties 
Assessment 
	: 
	The substance/mixture has no endocrine disrupting properties. 

	12.7. Other adverse effects 
Other adverse effects 
	: 
	Not classified as PMT or vPvM. 

	 
Effect on the ozone layer 
	: 
	No effect on the ozone layer. 

	Global warming potential [CO2=1] 
	: 
	1  

	Effect on global warming 
	: 
	When discharged in large quantities may contribute to the greenhouse effect. Contains greenhouse gas(es). 

	SECTION 13: Disposal considerations 
	
	


13.1. Waste treatment methods 
 	 	Discharge to atmosphere in large quantities should be avoided. 
Do not discharge into any place where its accumulation could be dangerous. 
Return unused product in original container to supplier. 
List of hazardous waste codes (from Commission 	: 16 05 05 : Gases in pressure containers other than those mentioned in 16 05 04. 
Decision 2000/532/EC as amended) 
13.2. Additional information 
 	 External treatment and disposal of waste should comply with applicable local and/or 
national regulations. 
SECTION 14: Transport information 
14.1. UN number or ID number 
In accordance with ADR / RID / IMDG / IATA / ADN 
	UN-No. 
14.2. UN proper shipping name 
	: 1013 

	Transport by road/rail/inland waterways 
(ADR/RID/ADN) 
	: CARBON DIOXIDE 

	Transport by air (ICAO-TI / IATA-DGR) 
	: Carbon dioxide 

	Transport by sea (IMDG) 
14.3. Transport hazard class(es) 
	: CARBON DIOXIDE 


[image: ]Labelling 	: 
  
	 
	 	2.2 : Non-flammable, non-toxic gases. 

	Transport by road/rail/inland waterways 
(ADR/RID/ADN) 
	 	 

	Class 
	: 2 

	Classification code 
	: 2A 

	Hazard identification number 
	: 20 

	Tunnel Restriction 
	: C/E - Tank carriage: Passage forbidden through tunnels of category C, D and E. Other carriage: Passage forbidden through tunnels of category E 

	Transport by air (ICAO-TI / IATA-DGR) 
	 	 

	Class / Div. (Sub. risk(s)) 
	: 2.2 

	Transport by sea (IMDG) 
	 	 

	Class / Div. (Sub. risk(s)) 
	: 2.2 

	Emergency Schedule (EmS) - Fire 
	: F-C 

	Emergency Schedule (EmS) - Spillage 
14.4. Packing group 
	: S-V 

	Transport by road/rail/inland waterways 
(ADR/RID/ADN) 
	: Not applicable. 

	Transport by air (ICAO-TI / IATA-DGR) 
	: Not applicable. 

	Transport by sea (IMDG) 14.5. Environmental hazards 
	: Not applicable. 

	Transport by road/rail/inland waterways 
(ADR/RID/ADN) 
	: None. 

	Transport by air (ICAO-TI / IATA-DGR) 
	: None. 

	Transport by sea (IMDG) 
14.6. Special precautions for user 
	: None. 

	Packing Instruction(s) 
	 	 

	Transport by road/rail/inland waterways 
(ADR/RID/ADN) 
	: P200. 

	Transport by air (ICAO-TI / IATA-DGR) 
	 	 

	     Passenger and Cargo Aircraft 
	: 200. 

	     Cargo Aircraft only 
	: 200. 

	Transport by sea (IMDG) 
	: P200. 

	 
	 	 


Special transport precautions 	Avoid transport on vehicles where the load space is not separated from the driver's compartment. 
Ensure vehicle driver is aware of the potential hazards of the load and knows what to do in the event of an accident or an emergency. 
Before transporting product containers: 
· Ensure there is adequate ventilation. 
· Ensure that containers are firmly secured. 
· Ensure valve is closed and not leaking. 
· Ensure valve outlet cap nut or plug (where provided) is correctly fitted. 
· Ensure valve protection device (where provided) is correctly fitted. 
14.7. Maritime transport in bulk according to IMO instruments 
 	 Not applicable. 
SECTION 15: Regulatory information 
15.1. Safety, health and environmental regulations/legislation specific for the substance or mixture EU-Regulations 
 
	Restrictions on use 
	: None. 

	Other information, restriction and prohibition regulations 
	: Not listed on the PIC list (Regulation EU 649/2012). 
Not listed on the POP list (Regulation EU 2019/1021). 

	Seveso Directive : 2012/18/EU (Seveso III) 
 
National regulations 
	: Covered. 

	Regulatory reference 
15.2. Chemical safety assessment 
	: Ensure all national/local regulations are observed. 

	 
	 A CSA does not need to be carried out for this product. 


SECTION 16: Other information 
	Indication of changes 
	: Revised safety data sheet in accordance with commission regulation (EU) No 453/2010. 


 
	Section 
	Changed item 
	Comments 

	 
	Supersedes version of 
	Modified 

	 
	Revision date 
	Modified 

	 
	Endocrine disrupting properties 
	Added 

	1 
	Relevant identified uses 
	Modified 

	2 
	Supplemental information 
	Added 

	2.3 
	Other hazards which do not result in classification 
	Modified 

	7 
	Safe handling of the gas receptacle 
	Modified 

	8 
	Regulatory reference 
	Added 

	8 
	Regulatory reference 
	Added 

	8 
	TGG-8u (OEL TWA) [ppm] 
	Added 

	8 
	Regulatory reference 
	Added 

	8 
	Local name 
	Added 

	8 
	Local name 
	Added 

	8 
	Local name 
	Added 

	8 
	OEL TWA 
	Added 

	8 
	OEL TWA 
	Added 

	8 
	TGG-8u (OEL TWA) 
	Added 

	8 
	OEL STEL 
	Added 

	8 
	OEL STEL 
	Added 

	8 
	OEL TWA 
	Added 

	8 
	OEL TWA 
	Added 

	8 
	Remark 
	Added 

	8 
	Regulatory reference 
	Added 

	8 
	Local name 
	Added 

	8 
	IOEL TWA [ppm] 
	Added 

	8 
	IOEL TWA 
	Added 

	8.2 
	Appropriate engineering controls 
	Modified 

	8.2 
	Respiratory protection 
	Modified 

	9 
	Particle characteristics 
	Added 

	9 
	Upper explosive limit (UEL) 
	Added 

	9 
	Lower explosive limit (LEL) 
	Added 

	9 
	Partition coefficient n-octanol/water (Log Kow) 
	Added 

	9 
	Density 
	Added 

	9 
	Partition coefficient n-octanol/water (Log Pow) 
	Modified 

	9 
	Melting point 
	Modified 

	9 
	Odour 
	Modified 

	9 
	Vapour pressure at 50°C 
	Modified 

	9 
	Viscosity, kinematic 
	Modified 

	9.1 
	Explosive limits (vol %) 
	Removed 

	9.1 
	Critical temperature 
	Modified 

	9.1 
	Decomposition temperature 
	Modified 

	11.1 
	Other information 
	Added 

	12.7 
	Other adverse effects 
	Modified 

	13.1 
	Waste treatment methods 
	Modified 

	14.6 
	Special provisions (ADR) 
	Modified 

	15 
	Seveso Directive : 2012/18/EU (Seveso III) 
	Modified 

	16 
	Abbreviations and acronyms 
	Modified 


 
	Abbreviations and acronyms 
	ATE - Acute Toxicity Estimate. 
CLP - Classification Labelling Packaging Regulation; Regulation (EC) No 1272/2008. REACH - Registration, Evaluation, Authorisation and Restriction of Chemicals Regulation (EC) No 1907/2006. 
EINECS - European Inventory of Existing Commercial Chemical Substances. 
CAS# - Chemical Abstract Service number. 
PPE - Personal Protection Equipment. 
LC50 - Lethal Concentration to 50 % of a test population. 
RMM - Risk Management Measures. 
PBT - Persistent, Bioaccumulative and Toxic. 
vPvB - Very Persistent and Very Bioaccumulative. 
STOT- SE : Specific Target Organ Toxicity - Single Exposure. 
CSA - Chemical Safety Assessment. 
EN - European Standard. 
UN - United Nations. 
ADR - Agreement concerning the International Carriage of Dangerous Goods by Road. 
IATA - International Air Transport Association. 
IMDG  code - International Maritime Dangerous Goods. 
RID - Regulations concerning the International Carriage of Dangerous Goods by Rail. 
WGK - Water Hazard Class. 
STOT - RE : Specific Target Organ Toxicity - Repeated Exposure. 
UFI : Unique Formula Identifier. 
ADN -International Carriage of Dangerous Goods by Inland Waterways. PROC -Process category 
. 
ERC – Environmental release category. 
PMT - Persistent, Mobile and Toxic. 
vPvM – very Persistent and very Mobile. 

	Training advice 
	: The hazard of asphyxiation is often overlooked and must be stressed during operator training. 
For more guidance, refer to  EIGA SL 01 “Dangers of Asphyxiation”, downloadable at http://www.eiga.eu.. 

	Further information 
	: Classification in accordance with the procedures and calculation methods of Regulation (EC) 1272/2008 (CLP). 
Key literature references and sources of data are maintained in EIGA doc 169 : 
'Classification and Labelling Guide', downloadable at  http://www.Eiga.eu . 


 
	Full text of H- and EUH-statements 
	

	Press. Gas (Liq.) 
	Gases under pressure : Liquefied gas 

	H280 
	Contains gas under pressure; may explode if heated. 


 
DISCLAIMER OF LIABILITY 	: Before using this product in any new process or experiment, a thorough material 
compatibility and safety study should be carried out. 
Details given in this document are believed to be correct at the time of going to press. Whilst proper care has been taken in the preparation of this document, no liability for injury or damage resulting from its use can be accepted. 
 
End of document 
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