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1 IDENTIFICATION OF THE SUBSTANCE / PREPARATION AND OF THE COMPANY / UNDERTAKING 
 

	Trade name 	 	 MSDS No. 	 	 
	Chemical Formula 	 
Company Identification

	 	 
 	 
 	 
 	 

 
 	 
	: Nitrogen (Liquid)	 
: AL007B 
: N2 
:  Janox BV
    Roggestraat 12
    8972 Krombeke
    +32(0) 57 30 98 40
    info@janox.be

	 
 2 HAZARDS IDENTIFICATION 
	
	


 
Classification of the substance 
· Physical Hazard 	 	 	 	: Gases under pressure  - Refrigerated liquefied gas 
· Health Hazard  	 	 	 	: no acute toxicity 
 
Label Elements 
· [image: ]Hazard Pictogram  	 	 	 
 
 
 
 
 
  
 
· Signal word 	 	 	 	: Warning 
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2 HAZARDS IDENTIFICATION (continued 	) 
 
· Hazard Statement  	 	 	: Contains refrigerated gas; may cause cryogenic burns or  
injury 
· Precautionary statements o Prevention    : Wear cold insulating gloves / face shield / eye protection 
· Response  	 	 	: Thaw frosted parts with lukewarm water. Do not rub affected  
area 
: Get immediate medical advice / attention 
· Storage 	 	 	 	: Store in a well ventilated area 
 
Other Hazard  	Other hazards 	 	 	 	: Contact with product may cause cold burns or frostbite. 
 	 	 	 	 	 	 	  In high concentration may cause asphyxiation. 
 
 
 
 3 COMPOSITION / INFORMATION ON INGREDIENTS 
	Substance / Preparation 	 	 	: Substance 
 
 Substance Name Contents CAS No. EC No.  Index No. Classification  Nitrogen (refrigerated)   100%  7727-37-9 231-783-9  --------    
 
 	Contains no other components or impurities which will influence the classification of the product. 
 
 
 
 4 FIRST AID MEASURES 
 
	First Aid Measures 
	
	

	- Inhalation 
	
	: In high concentrations may cause asphyxiation. Symptoms may include loss 
of mobility / consciousness. Victim may not be aware of asphyxiation 
Remove victim to uncontaminated area wearing self contained breathing apparatus. Keep victim warm and rested. Call a doctor. Apply artificial respiration if breathing stopped. 

	- Skin / Eye Contact 
	
	: Immediately flush eyes thoroughly with water for at least 15 minutes. 
In case of frostbite spray with water for at least 15 minutes. Apply a sterile dressing. Obtain medical assistance. 

	- Ingestion 	 
	 
	: Ingestion is not considered a potential route of exposure. 
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5 FIRE FIGHTING MEASURES 
 
	

		Flammable class 	 	 	 
Specific hazards 
	Hazardous Combustion Products 	 
Extinguishing media  
	- Suitable extinguishing media 	 
Specific methods 
Special protective equipment for fire fighters 
 
	: Non flammable 
: Exposure to fire may cause containers to rupture / explode : None 
:  All known extinguishants can be used. 
: If possible stop flow of product.  
Move away from   the container and cool with water from a protected position. If leaking do not spray water onto container. Water surrounding area (from protected position) to contain fire. 
: In confined space use self-contained breathing apparatus 

	6 ACCIDENTAL RELEASE MEASURES 	 
	

	 
Personal precautions 
 	 	 	 	 	 	 
	Environmental Precautions 	 	 
	Clean up methods 	 	 	 
 
	: Evacuate area 
Use protective clothing 
Wear self-contained breathing apparatus when entering area unless atmosphere is proved to be safe. Ensure adequate air ventilation. 
: Try to stop release. 
Prevent from entering sewers, basements and workpits, or any place where its accumulation can be dangerous. 
: Ventilate area. 

	 7 HANDLING AND STORAGE 
	


	Storage 	: Keep container below 50 degrees C in a well ventilated place. 
Handling 	: Suck back of water into the container must be prevented  	 	 	 	 	 	 	Do not allow backfeed into the container. 
Use only properly specified equipment which is suitable for this product, its supply pressure and temperature. Contact your gas supplier if in doubt.  
 	 	 	 	 	 	 	Refer to supplier’s container handling instructions.
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	8 EXPOSURE CONTROLS / PERSONAL PROTECTION 	 

	 
	Personal protection 	 	 	 
 	 	 	 	 	 	 
 
	: Ensure adequate ventilation. 
Protect eyes, face and skin from liquid splashes. 

	 
9 PHYSICAL AND CHEMICAL PROPERTIES 
 
	

		Physical state at 20 degrees C 	 
	Color  	 	 	 	 
	Odor 	 	 	 	 	 
	Molecular Weight 	 	 	 
	Melting point (degrees C) 	 	 
	Boiling point (degrees C) 	 	 
 
	Critical temperature (degrees C) 	 
	Vapor pressure, 20 degrees C  	 
	Relative density, gas (air =1)  	 
	Relative density, liquid (water = 1) 	 
	Solubility in water [mg/l] 	 	 
Other data 
	: Refrigerated liquefied gas. 
: Colorless liquid 
: No odor warning properties 
: 28 
: -210 
: -196 
: -147 
: Not Applicable 
: 0.97 
: 0.8 
: 20 
: Gas/vapor heavier than air. May accumulate in confined spaces, particularly at or below ground level. 

	 10 STABILITY AND REACTIVITY 
	


	Stability and reactivity  	 	 	: Stable under normal conditions. 
Liquid spillages can cause embrittlement of structural materials. 
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 11 TOXICOLOGICAL INFORMATION  
		Toxicity information 	 	 	 
	: No known toxicological effects from this product 

	 
12 ECOLOGICAL INFORMATION 
 
	

	Ecological effects information 
	: Can cause frost damage to vegetation. 

	 
13 DISPOSAL CONSIDERATIONS 
 
	

	General 
	: Do not discharge into any place where its accumulation could be dangerous.  
Contact supplier if guidance is required. 

	14 TRANSPORT INFORMATION 
	 


	UN No.  	 	 	 	 	: 1977 
 	H.I. nr  	 	 	 	 	: 22 
 	ADR / RID 	 	 	 	 	 
· Proper shipping name 	 	: Nitrogen, Refrigerated Liquid 
· ADR Class 	 	 	 	: 2 
· ADR / RID Classification code 	: 3 A  

· Labelling ADR 	 	 	:  
 
 
 
 
 
 
 
 
 2.2: Non flammable, non toxic gas. 
 
 
Other transport information : Avoid transport on vehicles where the load space is not separated from the driver’s compartment 
	 	Ensure vehicle driver is aware of the potential hazards of the 
load and knows what to do in the event of an accident or an emergency. 
	 	Before transporting product containers: 
· Ensure that containers are firmly secured. 
· Ensure cylinder valve is closed and not leaking. 
· Ensure valve outlet cap nut or plug (where provided) is correctly fitted. 
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	14 TRANSPORT INFORMATION (continued) 
	- 	 
- 	 


 
· Ensure valve protection device (where provided) is correctly fitted. 
· Ensure there is adequate ventilation. 
· Compliance with applicable regulations 
 
	15 REGULATORY INFORMATION 
	 

	 
	EC Classification 	 	 	 
	EC Labeling 	 	 	 	 
· Symbol (s) 	 	 	 	 
· R Phrase (s)  	 	 	 
· S Phrase (s)  	 	 	 
	: Not included in Annex I. 
Not classified as dangerous preparation / substance : No EC labeling required. 
: None 
: None 
: None 

	 
16 OTHER INFORMATION  	 
	


· May cause frostbite. 
· Keep container in a well-ventilated place. 
· Do not breathe the gas. 
· Ensure all national / local regulations are observed. 
· Asphyxiant in high concentrations. 
· The hazard of asphyxiation is often overlooked and must be stressed during operator training. 
· This Material Safety Data Sheet has been established in accordance with the applicable European Directives and applies to all countries that have translated the Directives in their national laws. 
· Before using this product in any new process or experiment, a thorough material compatibility and safety study should be carried out. 
· Details given in this document are believed to be correct at the time of going to press. Whilst proper care has been taken in the preparation of this document, no liability for injury or damage resulting from its use can be accepted. 
 
Recommended uses and restrictions: This MSDS is for information purposes only and is subject to change without prior notice. [Prior to purchase of products, please contact your local AIR LIQUIDE office for complete MSDS (with Manufacturer’s name and emergency phone number)]. 
 
 

End of Document 
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